# 2022 Jeep® Gladiator

## FEATURE AVAILABILITY

S = Standard. O = Optional. P = Part of package. NA = Not available.   
Note: some features and/or applications may be late availability.

### ENGINES / TRANSMISSIONS

| ENGINES | TRANSMISSIONS | Sport | Overland | Mojave | Rubicon |
| --- | --- | --- | --- | --- | --- |
| Pentastar 3.6-liter V-6 SMPI | Six-speed manual | S | S | S | S |
| Pentastar 3.6-liter V-6 SMPI | Eight-speed automatic | O | O | O | O |
| 3.0-Liter EcoDiesel V-6 | Eight-speed automatic | O | O | NA | O |

### MECHANICAL / CAPABILITY

| MECHANICAL / CAPABILITY | Sport | Overland | Mojave | Rubicon |
| --- | --- | --- | --- | --- |
| Axle Ratios |  |  |  |  |
| 3.73:1 | S | S | NA | NA |
| 4.10:1 | O | NA | S | S |
| Axles |  |  |  |  |
| 3rd generation Dana 44 heavy-duty solid front | S | S | NA | NA |
| 3rd generation Dana 44 heavy-duty solid rear | S | S | NA | NA |
| 3rd generation Dana 44 heavy-duty solid front (wide track) | O | NA | S | S |
| 3rd generation Dana 44 heavy-duty solid rear (wide track) | O | NA | S | S |
| Differentials |  |  |  |  |
| Trac-Lok limited-slip, rear | O | O | NA | NA |
| Tru-Lok front, electronic remote locking | NA | NA | NA | S |
| Tru-Lok rear, electronic remote locking | NA | NA | S | S |
| Sway-bar disconnect — electronically controlled, front | NA | NA | NA | S |
| Suspension |  |  |  |  |
| FOX monotube shocks | NA | NA | NA | S |
| FOX internal bypass, external reservoir shocks | NA | NA | S | NA |
| FOX front hydraulic jounce bumpers | NA | NA | S | NA |
| Trailer-sway control | S | S | S | S |
| Transfer Case |  |  |  |  |
| Transfer case/4WD system — Command-Trac NV241,  part-time, shift-on-the-fly transfer case | S | S | S | NA |
| Selec-Trac full-time transfer case (2.72:1) | O | O | O | NA |
| Rock-Trac NV241 OR, part-time, shift-on-the-fly transfer case; 4:1 low-gear ratio | NA | NA | NA | S |
| Rock-Trac NV241 OR, full-time, shift-on-the-fly transfer case; 4:1 low-gear ratio | NA | NA | NA | O |

### TOWING AND HAULING

| TOWING AND HAULING | Sport | Overland | Mojave | Rubicon |
| --- | --- | --- | --- | --- |
| Towing |  |  |  |  |
| Four-pin and seven-pin trailer wiring | S | S | S | S |
| Class II bumper hitch | S | S | S | S |
| Class IV receiver hitch | P | P | P | P |
| Truck Bed |  |  |  |  |
| 5-foot steel box | S | S | S | S |
| Damped three-position tailgate | S | S | S | S |
| Cargo lights | S | S | S | S |
| Spray-in bedliner | O | O | O | O |
| Roll-up tonneau cover | O | O | O | O |
| 115-volt power outlet | P | P | P | P |
| Adjustable rail-based tie-down system | P | P | P | P |

### EXTERIOR

| EXTERIOR | Sport | Overland | Mojave | Rubicon |
| --- | --- | --- | --- | --- |
| Doors |  |  |  |  |
| Full-metal doors with roll-up windows | S | NA | NA | NA |
| Full-metal doors with power windows | O | S | S | S |
| Half doors | P | P | P | P |
| Door Locks |  |  |  |  |
| Manual door locks — full door | S | NA | NA | NA |
| Power door locks (speed-sensitive locking) —  door-mounted switches | O | S | S | S |
| Fender Flares |  |  |  |  |
| Black, one-piece | S | NA | NA | NA |
| Two-piece — body-color insert | O | S | NA | NA |
| Two-piece, high clearance — black | NA | NA | S | S |
| Two-piece, high clearance — body-color insert | NA | NA | O | O |
| Forward-facing off-road camera | NA | O | O | O |
| Glass |  |  |  |  |
| Standard | S | NA | NA | NA |
| Deep-tinted sunscreen rear and quarter windows | O | S | S | S |
| Corning Gorilla Glass windshield | O | O | O | O |
| Grille |  |  |  |  |
| Body-color grille | S | NA | NA | NA |
| Body-color grille — Overland accent throats  and headlamp rings | NA | S | NA | NA |
| Body-color grille — Mojave and Rubicon accent throats and headlamp rings | NA | NA | S | S |
| Lighting |  |  |  |  |
| Halogen headlamps | S | S | S | S |
| LED reflector headlamps (packaged with LED Lighting Group) | P | P | P | P |
| Fog lamps | S | S | S | S |
| LED fog lamps (packaged with LED Lighting Group) | P | P | P | P |
| Automatic headlamps | O | S | S | S |
| Mirrors |  |  |  |  |
| Mold-in color manual folding mirrors | S | S | S | S |
| Standard mirrors — no power | S | NA | NA | NA |
| Power-heated mirrors | O | S | S | S |
| Blind-spot Monitoring indicator inside mirrors | P | P | P | P |
| Rock rails — Cab and bed, black, painted steel, heavy-duty, and protective | NA | NA | NA | S |
| Rock rails — Cab, black, painted steel, heavy-duty,  and protective | NA | NA | S | NA |
| Side steps — tubular, diamond plate surface pattern | O | S | NA | NA |
| Skid Plates |  |  |  |  |
| Fuel tank and transfer case | S | S | S | S |
| Front skid plate/brush guard | NA | NA | S | S |
| Tires |  |  |  |  |
| 32-in. — all-season tires, 245/75 R17 BSW Bridgestone  Dueler H/T | S | NA | NA | NA |
| 32-in. — all-terrain tires, 245/75 R17 BSW Bridgestone  Dueler A/T | O | NA | NA | NA |
| 33-in. — all-terrain tires, 285/70R17 Falken Wildpeak A/T | NA | NA | S | S |
| 32-in. — all-season tires, 255/70R18 Bridgestone Dueler H/T | NA | S | NA | NA |
| 32-in. — all-terrain tires, 255/70R18 Bridgestone Dueler A/T | NA | O | NA | NA |
| 33-in. — mud-terrain tires, 285/70R17 Falken Wildpeak M/T | NA | NA | O | O |
| Tops |  |  |  |  |
| Sunrider folding soft-top with sunroof feature | S | S | S | S |
| Premium Sunrider soft-top | O | O | O | O |
| Freedom Top three-piece modular hardtop with rear defroster, sliding rear window and Freedom Panel storage bag | O | O | O | O |
| Body-color three-piece hardtop | NA | O | O | O |
| Dual Top Group (includes premium Sunrider) | O | O | O | O |
| Mopar Sunrider soft-top for hardtop | O | O | O | O |
| Tow hooks — two front, one rear | S | S | NA | NA |
| Tow hooks — two front, two rear | NA | NA | S | S |
| Wheels |  |  |  |  |
| 17-in. full-face steel wheels painted Low Gloss Black | S | NA | NA | NA |
| 17-in. aluminum fully painted High Gloss Tech Silver wheels | O | NA | NA | NA |
| 17-in. aluminum fully painted High Gloss Black wheels (Sport S) | O | NA | NA | NA |
| 18-in. aluminum polish/painted Granite Crystal  wheels (Overland) | NA | S | NA | NA |
| 17-in. aluminum painted Low Gloss Black | NA | NA | S | NA |
| 17-in. aluminum polish/painted Low Gloss Black | NA | NA | O | NA |
| 17-in. aluminum polish/painted Granite Crystal wheels (Rubicon) | NA | NA | NA | S |
| Optional 17-in. aluminum polish/painted Mid-gloss  Black wheels (Rubicon) | NA | NA | NA | O |
| Windows (manual) |  |  |  |  |
| Full door | S | NA | NA | NA |
| Power windows (front and rear), driver and passenger  one-touch down | O | S | S | S |

### INTERIOR

| INTERIOR | Sport | Overland | Mojave | Rubicon |
| --- | --- | --- | --- | --- |
| Air Conditioning |  |  |  |  |
| Air conditioning — manual, single zone | S | NA | NA | NA |
| Air conditioning with automatic temperature control —  dual zone | P | S | S | S |
| Cabin air filter — dual zone | P | S | S | S |
| Console — full-floor with front and rear cup holders,  locking storage and armrest | S | S | S | S |
| Floor heat ducts — rear | S | S | S | S |
| Floor Mats |  |  |  |  |
| Front and rear | S | S | S | S |
| Mopar slush mats | O | O | O | O |
| Lighting |  |  |  |  |
| LED front cup holder | S | S | S | S |
| LED rear cup holder | S | S | S | S |
| LED overhead courtesy lamp | S | S | S | S |
| LED door bezel ambient lamp | S | S | S | S |
| LED footwell courtesy — functional | S | S | S | S |
| LED ambient footwell lamp — mood/accent light | NA | S | S | S |
| LED center console ambient lamp | NA | NA | S | S |
| Passive entry | P | S | S | S |
| Push button start | S | S | S | S |
| Remote Keyless Entry with mechanical flip key | O | S | S | S |
| Remote start system | P | O/P | O/P | O/P |
| Lockable rear behind-seat storage | S | S | S | S |
| Rear under-seat storage | S | S | S | S |
| Lockable and removable storage bin under rear seat | P | P | P | P |
| Auxiliary electrical switches – four programmable switches, heavy-duty 240-amp alternator | O | O | O | O |
| Seating |  |  |  |  |
| Cloth seats | S | S | NA | NA |
| Premium cloth seats | NA | NA | S | S |
| Leather-trimmed seats | NA | O | O | O |
| Heated front seats | P | P | P | P |
| Driver seat — six-way manual (fore/aft, recline, height adjust) | S | S | S | S |
| Front passenger seat — four-way manual (fore/aft, recline) | S | S | S | S |
| Two-way lumbar (driver only) | S | S | S | S |
| Tilt/telescoping steering column — manual | S | S | S | S |
| Steering Wheel |  |  |  |  |
| Base (urethane) | S | NA | NA | NA |
| Leather wrapped | O | S | NA | S |
| Competition-inspired leather wrapped | NA | NA | S | NA |
| Mounted audio controls | S | S | S | S |
| EVIC controls | S | S | S | S |
| Heated steering wheel | P | P | P | P |
| Speed and cruise control | S | S | S | S |
| Universal garage door opener | P | S | S | S |
| Hardtop headliner | O | O | O | O |
| Wash-out interior with removable carpet and drain plugs | S | S | S | S |

### UCONNECT / MULTIMEDIA

| UCONNECT / MULTIMEDIA | Sport | Overland | Mojave | Rubicon |
| --- | --- | --- | --- | --- |
| Audio System |  |  |  |  |
| Eight speakers | S | NA | NA | NA |
| Nine Alpine speakers with all-weather subwoofer  and 552-watt amplifier | O/P | S | S | S |
| Auxiliary power, 115-volt outlet in center console | P | S | S | S |
| Media hub (one full-function USB and auxiliary port) | S | S | S | S |
| Power outlet, 12-volt, instrument panel | S | S | S | S |
| Radio with Uconnect 4 with 7-in. display | S | NA | NA | NA |
| Radio with Uconnect 4C NAV with 8.4-in. display | P | S | S | S |
| Removable Bluetooth wireless speaker | O | O | O | O |
| SiriusXM Radio — includes a six-month trial subscription | O | S | S | S |
| SiriusXM Guardian Connected Services — includes one-year trial | P | S | S | S |
| SiriusXM Travel Link — includes five-year trial subscription | P | S | S | S |
| SiriusXM Traffic Plus — includes five-year trial subscription | P | S | S | S |
| Uconnect Voice Command — hands-free calling with address book and Bluetooth | S | S | S | S |
| USB — fully functional in center console | S | S | S | S |
| Two USBs and two USB-C in back of center console | P | S | S | S |

### SAFETY & SECURITY

| SAFETY & SECURITY | Sport | Overland | Mojave | Rubicon |
| --- | --- | --- | --- | --- |
| Advanced multistage front airbags | S | S | S | S |
| Adaptive cruise control | P | P | P | P |
| Antilock braking system with Hydraulic Assist Braking | S | S | S | S |
| Blind-spot Monitoring | P | P | P | P |
| Driver and front passenger seat belt alert (all markets) | S | S | S | S |
| Forward Collision Warning | P | P | P | P |
| Electronic Roll Mitigation | S | S | S | S |
| Electronic stability control — includes hydraulic assist brake booster and traction control | S | S | S | S |
| Front passenger seat Occupant Detection System | S | S | S | S |
| Hill-start Assist | S | S | S | S |
| Rear Child Seat Anchors — LATCH | S | S | S | S |
| Rear Park Assist | P | P | P | P |
| Rear backup camera with dynamic gridlines | S | S | S | S |
| Selec-Speed Control (packaged with eight-speed automatic transmission) | P | P | P | P |
| Sentry Key antitheft engine immobilizer | S | S | S | S |
| Supplemental front seat side airbag | S | S | S | S |
| Tire-pressure Monitoring | S | S | S | S |
| Vehicle theft alarm — protects doors and liftgate | O | S | S | S |

### PACKAGES / EQUIPMENT GROUPS

| PACKAGES / EQUIPMENT GROUPS | Sport | Overland | Mojave | Rubicon |
| --- | --- | --- | --- | --- |
| Jeep Active Safety Group — includes Rear Park Assist, Blind-spot Monitoring and LED taillamps | O | O | O | O |
| Jeep Advanced Safety Group — includes adaptive cruise control and forward collision warning | O | O | O | O |
| Infotainment Group — includes 8.4-in. VP4 radio with NAV, inside electro-chromatic rearview mirror, SOS Call located on the header above rearview mirror and nine-speaker premium audio system with all-weather subwoofer | O | S | S | S |
| Cold Weather Group — includes heated front seats, heated steering wheel and remote start | O | O | O | O |
| Trail Rail Cargo Management Group — includes three box rails, four anchor pods, 115-volt bed power outlet and lockable rear under-seat storage bin | O | O | O | O |
| Black Three-piece Hardtop Group — includes black three-piece hardtop with Freedom panels, rear window defroster and sliding rear window | O | O | O | O |
| Body-color Three-piece Hardtop Group — includes body-color three-piece hardtop with Freedom panels, rear window defroster and sliding rear window | NA | O | O | O |
| LED Lighting Group — includes LED headlamps with round signature lighting, LED front fog lamps, LED daytime running lamps, LED Park Turn and LED taillamps | NA | O | O | O |
| LED Headlamp and Fog Lamp Package | O | NA | NA | NA |
| Trailer Tow Group — includes heavy-duty 240-amp alternator, Class IV hitch receiver and heavy-duty cooling | O | O | O | O |
| Max Trailer Tow Group — includes heavy-duty 240-amp alternator, Class IV hitch receiver heavy-duty cooling, wide-track axles with 4.10:1 axle ratio | O | NA | NA | NA |
| Convenience Group — includes remote start and universal garage door opener | O | NA | NA | NA |
| Technology Group — includes 7-in. thin-film transistor (TFT) cluster, passive entry, satellite radio and automatic temperature control with dual zone | O | NA | NA | NA |
| Rubicon heavy metal winch-capable front bumper — includes steel front bumper with removable endcaps | NA | NA | NA | O |

###